Invitation to tender text

---------------------------------------------------------------------------------------------------------------------

Remotely controlled KNX presence detector with 180° field of detection for wall mounting
Special product features: KNX functions: Twilight switch, motion direction detection function, brightness detection via object, light-dependent motion detection; 
User interface: IR remote control, ETS-Software
Control system: KNX
Installation type: Flush-mounted/Device socket Ø 68 mm
Installation position: Wall
Dimensions: Length 70 mm x Width 70 mm x Height/Depth 55 mm
Installation dimension: Installation depth: 25 mm, Ø 60 mm
Weight: 50 g
Protection type: IP20, IP44 depending on cover (order separately)
Protection class: III
Permissible ambient temperature: 5 °C...+50 °C
Relative humidity: 5–93 %, non-condensing
Colour: white, similar to RAL 9010
Nominal voltage: 29 – 31 V DC
Power consumption: 0,2 W
Detection angle: 180° horizontal, 60° vertical
Detection range diagonally: Ø 16 m
Detection range head-on: Ø 12 m
Detection range presence: Ø 8 m
Field of detection: up to 101 m²
Recommended installation height: 1,1 m
Max. mounting height: 2,2 m
Level of brightness: 5–2000 lx
Number of light channels: 2
Slave input: true
Mode: Semi-automatic, Fully automatic
Constant light control: false
Switching delay from "dark to light": 300 s
Switching delay from "light to dark": 30 s
Switching capacity channel 1: Bus system
Switch-off delay time: 60 s...30 min (adjustable in steps)
Impulse mode: false
Push button input: false