ESYLUX / Outdoor automation / Motion detectors

EM10025211 - MD 120 weiß Bewegungsmelder

ESYLUX MD 120 white
Motion detector with 120° field of detection for convenient lighting control
Special product features: <ul><li>One-hand plug-in base</li><li>Zero-cross switching</li></ul>
User interface: Adjusting controller
Control system: ON/OFF
Installation type: Surface mounting
Installation position: Wall
Dimensions: Length 102 mm x Width 74 mm x Height/Depth 81 mm
Weight: 184 g
Protection type: IP44
Protection class: II
Permissible ambient temperature: -25 °C...+55 °C
Relative humidity: 5&nbsp;–&nbsp;95 %, non-condensing
Colour: white, similar to RAL 9010
Nominal voltage: 230 V AC / 50 Hz
In-rush current: 30 A / 20 ms
Power consumption: 0,5 W
Detection angle: 120° sensor horizontally rotatable +/- 90°
Detection range diagonally: r 12 m
Detection range head-on: r 5 m
Field of detection: up to 151 m²
Recommended installation height: 2,5 m
Max. mounting height: 2,5 m
Level of brightness: 10&nbsp;–&nbsp;2000 lx
Number of light channels: 1
Slave input: false
Constant light control: false
Switching delay from "dark to light": 0 s
Switching delay from "light to dark": 0 s
Switching capacity channel 1: 230 V AC 50 Hz,
1000 W/4.5 A (cos phi = 1),
500 VA/2.25 A (cos phi = 0.5)
Switch contact: make contact / non-floating
Switch-off delay time: 10 s...15 min (adjustable in steps)
Impulse mode: false
Push button input: false